Copyright 2021 ADVANCED MICRO DEVICES, INC. All Rights Reserved. 

AMD RAID controller driver distribution list
Revision: 9.3.0.00296
Build date: 08/18/2021
OS: Windows10 x64, Windows11 x64

Driver package:
WIN10\x64\ NVMe_DID (AMD Non-Volatile Memory Express Device ID files)
Supported AMD processors:
•	AMD Ryzen™ 3000 Series Desktop Processors with Radeon™ Graphics 
•	AMD Ryzen™ 4000 Series Desktop Processors with Radeon™ Graphics
•	AMD Ryzen™ 5000 Series Desktop Processors with Radeon™ Graphics
•	AMD Ryzen™ 4000 Series Mobile Processors with Radeon™ Graphics
•	AMD Ryzen™ 5000 Series Mobile Processors with Radeon™ Graphics
•	3rd Gen AMD Ryzen™ Threadripper™ Processors

WIN10\x64\NVMe_CC (Non-Volatile Memory Express Controller Class Code files) 
Supported AMD processors:
•	AMD Ryzen™ 1000 Series Desktop Processors
•	AMD Ryzen™ 2000 Series Desktop Processors
•	AMD Ryzen™ 3000 Series Desktop Processors
•	AMD Ryzen™ 5000 Series Desktop Processors
•	AMD Ryzen™ 2000 Series Desktop Processors with Radeon™ Graphics 
•	1st Gen AMD Ryzen™ Threadripper™ Processors
•	2nd Gen AMD Ryzen™ Threadripper™ Processors
		
WIN10\x64\RAID_SATA
•	Supports all raid enabled Ryzen AMD processors (SATA only)

Note:
•	RAID SATA is not supported AMD Ryzen™ Mobile Processors with Radeon™ Graphics 
•	AMD Ryzen™ 4000 and 5000 Series Mobile Processors with Radeon™ Graphics supports NVMe in RAID0 / Raid1 only
•	RAID5 is only supported on 3rd and 4th Gen AMD Ryzen™ Threadripper™ Processors
•	Driver files in folder NVMe_CC and NVMe_DID enable both NVMe (Non-Volatile Memory Express) devices and SATA devices to be configured in RAID.

AMD-RAID binary file name:
•	rcraid.cat, rcraid.inf, rcraid.sys
•	rccfg.cat, rccfg.inf, rccfg.sys
•	rcbottom.cat, rcbottom.inf, rcbottom.sys

Known issues
•	No support for 2 ODDs on the same port of 2 different controllers.
•	HyperX card is dropped during ACPI 
•	Performance issue on some specific drives
•	With 11 PCIe NVMe SSD's system boot to OS may fail.
•	RS5x64 OS taking long time to load the driver.
•	OS Installation may fail when OS installed on other than first RAID array.

Revision History
9.3.0.00296
•	Fix for OS installation issue with Max configuration.
•	Fix for F11 OS Reset Issue after windows major updates.
9.3.0.00295
•	Fix for Bugcheck 7B (BSOD) while running Reboot cycles.
•	Fix for F11 OS Reset Issue.

9.3.0.00266
•	Fix for hibernate performance on HDD
•	Fix for BSOD during clear metadata
•	Fix for SMART info on specific Model of NVMe

9.3.0.00245
•	Fix for BSOD issue while installing OS with 8xNVMe and 3xHDD.

9.3.0.00237
•	Fix for Negative (-ve) reading for temperature value.
•	Fix for Power Hours and Power cycle value.

9.3.0.00230
•	Support to get S.M.A.R.T information for NVME and SATA Devices
•	Check for “Smart get Command set” under rcadm.exe help for commands.
•	Eg: 
•	rcadm.exe –M –sg –o 
•	rcadm.exe –M –sg –o –d

9.3.0.00206
•	Fix for hibernate resume time on RAID-5 HDD.
•	Fix 0x9f issue during S3 when multiple creates are active.

9.3.0.00198
•	Added Clear metadata feature to clear the RAID metadata.
•	updated user guide with clear metadata changes.